|  |  |
| --- | --- |
| 3GPP TR 38.717-01-01 V17.0.0 (2022-06) | |
| Technical Report | |
| 3rd Generation Partnership Project;  Technical Specification Group Radio Access Networks;  NR intra band Carrier Aggregation for xCC DL/yCC UL  including contiguous and non-contiguous spectrum (x>=y)  (Release 17) | |
|  | |
| *5G-logo_175px* | 3GPP-logo_web |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 6

1 Scope 8

2 References 8

3 Definitions of terms, symbols and abbreviations 8

3.1 Terms 8

3.2 Symbols 8

3.3 Abbreviations 8

4 Background 8

4.1 TR maintenance 9

5 Intra-Band Contiguous Carrier Aggregation FR1: Specific Band Combination Part 9

5.1 CA\_n96 DL\_n96UL 9

5.1.1 Channel bandwidths per operating band for CA 9

5.1.2 UE co-existence studies 9

5.1.3 REFSENS 9

5.2 CA\_2DL\_n2B\_1UL\_n2A 9

5.2.1 Channel bandwidths per operating band for CA 9

5.2.2 UE maximum output power for Intra-band contiguous CA 10

5.2.3 UE additional maximum output power reduction for CA 10

5.2.4 Spurious emissions for UE co-existence for intra-band contiguous CA 10

5.2.5 Reference sensitivity power level for Intra-band contiguous CA 10

5.2.6 In-band blocking 10

5.2.7 Out-of-band blocking 11

5.2.8 Narrow band blocking 11

5.3 CA\_2DL\_n25B\_1UL\_n25A 11

5.3.1 Channel bandwidths per operating band for CA 11

5.3.2 UE maximum output power for Intra-band contiguous CA 12

5.3.3 UE additional maximum output power reduction for CA 12

5.3.4 Spurious emissions for UE co-existence for intra-band contiguous CA 12

5.3.5 Reference sensitivity power level for Intra-band contiguous CA 12

5.3.6 In-band blocking 12

5.3.7 Out-of-band blocking 13

5.3.8 Narrow band blocking 13

5.4 CA\_2DL\_n77B\_1UL\_n77A 13

5.4.1 Channel bandwidths per operating band for CA 13

5.4.2 UE maximum output power for Intra-band contiguous CA 14

5.4.3 UE additional maximum output power reduction for CA 14

5.4.4 Spurious emissions for UE co-existence for intra-band contiguous CA 14

5.4.5 Reference sensitivity power level for Intra-band contiguous CA 14

5.4.6 In-band blocking 14

5.4.7 Out-of-band blocking 14

5.4.8 Narrow band blocking 14

5.5 CA\_2DL\_n40B\_2UL\_n40B 14

5.5.1 Channel bandwidths per operating band for CA 14

5.5.2 UE maximum output power for Intra-band contiguous CA 15

5.5.3 UE additional maximum output power reduction for CA 15

5.5.4 Spurious emissions for UE co-existence for intra-band contiguous CA 15

5.5.5 Reference sensitivity power level for Intra-band contiguous CA 16

5.5.6 In-band blocking 16

5.5.7 Out-of-band blocking 16

5.5.8 Narrow band blocking 16

5.6 CA\_2DL\_n3B\_1UL\_n3A 16

5.6.1 Channel bandwidths per operating band for CA 16

5.6.2 UE maximum output power for Intra-band contiguous CA 16

5.6.3 UE additional maximum output power reduction for CA 16

5.6.4 Spurious emissions for UE co-existence for intra-band contiguous CA 16

5.6.5 Reference sensitivity power level for Intra-band contiguous CA 17

5.6.6 In-band blocking 17

5.6.7 Out-of-band blocking 17

5.6.8 Narrow band blocking 18

5.7 CA\_2DL\_n38B\_1UL\_n38A 18

5.7.1 Channel bandwidths per operating band for CA 18

5.7.2 UE maximum output power for Intra-band contiguous CA 18

5.7.3 UE additional maximum output power reduction for CA 19

5.7.4 Spurious emissions for UE co-existence for intra-band contiguous CA 19

5.7.5 Reference sensitivity power level for Intra-band contiguous CA 19

5.7.6 In-band blocking 19

5.7.7 Out-of-band blocking 19

5.7.8 Narrow band blocking 20

6 Intra-Band Non-Contiguous Carrier Aggregation FR1: Specific Band Combination Part 20

6.1 CA\_2DL\_n71(2A)\_1UL\_n71A 20

6.1.1 Channel bandwidths per operating band for CA 20

6.1.2 UE co-existence studies 20

6.1.3 REFSENS 20

6.2 CA\_2DL\_n2(2A)\_1UL\_n2A 21

6.2.1 Channel bandwidths per operating band for CA 21

6.2.2 Co-existence studies 21

6.2.3 REFSENS 21

6.3 CA\_2DL\_n5(2A)\_1UL\_n5A 22

6.3.1 Channel bandwidths per operating band for CA 22

6.3.2 UE co-existence studies 22

6.3.3 REFSENS 22

6.4 CA\_3DL\_n77(3A)\_1UL\_n77A 23

6.4.1 Channel bandwidths per operating band for CA 23

6.4.2 Co-existence studies 23

6.4.3 REFSENS 23

6.5 CA\_2DL\_n96(2A)\_1UL\_n96A 23

6.5.1 Channel bandwidths per operating band for CA 23

6.5.2 UE co-existence studies 23

6.5.3 REFSENS 23

6.6 CA\_2DL\_n96(3A)\_1UL\_n96A 24

6.6.1 Channel bandwidths per operating band for CA 24

6.6.2 UE co-existence studies 24

6.6.3 REFSENS 24

6.7 CA\_2DL\_n96(4A)\_1UL\_n96A 24

6.7.1 Channel bandwidths per operating band for CA 24

6.7.2 UE co-existence studies 24

6.7.3 REFSENS 24

6.8 CA\_2DL\_n12(2A)\_1UL\_n12A 25

6.8.1 Channel bandwidths per operating band for CA 25

6.8.2 UE maximum output power for Intra-band contiguous CA 25

6.8.3 UE additional maximum output power reduction for CA 25

6.8.4 Spurious emissions for UE co-existence for intra-band contiguous CA 25

6.8.5 Reference sensitivity power level for Intra-band contiguous CA 25

6.8.6 In-band blocking 26

6.8.7 Out-of-band blocking 26

6.8.8 Narrow band blocking 26

6.9 CA\_2DL\_n25(2A)\_1UL\_n25A CA\_3DL\_n25(3A)\_1UL\_n25A 26

6.9.1 Channel bandwidths per operating band for CA 26

6.9.2 REFSENS 27

6.10 CA\_2DL\_n41(2A)\_1UL\_n41A CA\_2DL\_n41(A-C)\_1UL\_n41A CA\_3DL\_n41(3A)\_1UL\_n41A 27

6.10.1 Channel bandwidths per operating band for CA 27

6.10.2 REFSENS 27

6.11 CA\_2DL\_n1(2A)\_1UL\_n1A 28

6.11.1 Channel bandwidths per operating band for CA 28

6.11.2 Co-existence studies 28

6.11.3 REFSENS 28

7 Intra-Band Contiguous Carrier Aggregation FR2: Specific Band Combination Part 28

7.1 CA\_xDL\_a\_yUL\_b 28

7.1.1 Channel bandwidths per operating band for CA 28

7.1.2 UE co-existence studies 28

8 Intra-Band Non-Contiguous Carrier Aggregation FR2: Specific Band Combination Part 28

8.1 CA\_xDL\_a-a\_yUL\_b-b 28

8.1.1 Channel bandwidths per operating band for CA 28

8.1.2 UE co-existence studies 29

Annex A - Change history 30

# Foreword

This Technical Report has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

In the present document, modal verbs have the following meanings:

**shall** indicates a mandatory requirement to do something

**shall not** indicates an interdiction (prohibition) to do something

The constructions "shall" and "shall not" are confined to the context of normative provisions, and do not appear in Technical Reports.

The constructions "must" and "must not" are not used as substitutes for "shall" and "shall not". Their use is avoided insofar as possible, and they are not used in a normative context except in a direct citation from an external, referenced, non-3GPP document, or so as to maintain continuity of style when extending or modifying the provisions of such a referenced document.

**should** indicates a recommendation to do something

**should not** indicates a recommendation not to do something

**may** indicates permission to do something

**need not** indicates permission not to do something

The construction "may not" is ambiguous and is not used in normative elements. The unambiguous constructions "might not" or "shall not" are used instead, depending upon the meaning intended.

**can** indicates that something is possible

**cannot** indicates that something is impossible

The constructions "can" and "cannot" are not substitutes for "may" and "need not".

**will** indicates that something is certain or expected to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**will not** indicates that something is certain or expected not to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**might** indicates a likelihood that something will happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

**might not** indicates a likelihood that something will not happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

In addition:

**is** (or any other verb in the indicative mood) indicates a statement of fact

**is not** (or any other negative verb in the indicative mood) indicates a statement of fact

The constructions "is" and "is not" do not indicate requirements.

# 1 Scope

The present document is a technical report for NR Intra-band Carrier Aggregation Rel-17 for xDL/yUL including contiguous and non-contiguous spectrum under Rel-17 time frame. The purpose is to gather the relevant background information and studies in order to address NR Intra-band Carrier Aggregation requirements for the Rel-17 band combinations requested by proponents and captured in the WID..

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] RP-200663, “New WID: NR intra band Carrier Aggregation for xCC DL/yCC UL including contiguous and non-contiguous spectrum (x>=y)”, RAN#88-e

# 3 Definitions of terms, symbols and abbreviations

## 3.1 Terms

For the purposes of the present document, the terms given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

**example:** text used to clarify abstract rules by applying them literally.

## 3.2 Symbols

For the purposes of the present document, the following symbols apply:

<symbol> <Explanation>

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

<ABBREVIATION> <Expansion>

# 4 Background

The present document is a technical report for NR Intra-band Carrier Aggregation under Rel-17 timeframe. The document covers each band combination specific issues (i.e. one sub-clause defined per band combination)

## 4.1 TR maintenance

A single company is responsible for introducing all approved TPs in the current TR, i.e. TR editor. However, it is the responsibility of the contact person of each band combination to ensure that the TPs related to the band combination have been implemented.

# 5 Intra-Band Contiguous Carrier Aggregation FR1: Specific Band Combination Part

## 5.1 CA\_n96 DL\_n96UL

### 5.1.1 Channel bandwidths per operating band for CA

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **NR CA configuration / Bandwidth combination set** | | | | | | | | |
| **NR CA configuration** | **Uplink NR CA  configurations** | **channel bandwidths  for carrier [MHz]** | **channel bandwidths  for carrier [MHz]** | **channel bandwidths  for carrier [MHz]** | **channel bandwidths  for carrier [MHz]** | **channel bandwidths  for carrier [MHz]** | **Maximum aggregated  bandwidth** | **Bandwidth combination set** |
| CA\_n96B | CA\_n96B | 20, 40 | 20, 40, 60, 80 |  |  |  | 100 | 0 |
| CA\_n96C | CA\_n96C | 80 | 40, 60, 80 |  |  |  | 160 | 0 |
| CA\_n96D | - | 80 | 80 | 60, 80 |  |  | 240 | 0 |
| CA\_n96E | - | 80 | 80 | 80 | 80 |  | 320 | 0 |

### 5.1.2 UE co-existence studies

There are no co-existence issues for this combination.

### 5.1.3 REFSENS

Considering the receiver design for the higher operation frequency with for the band. And for CA\_n96E, there may be gain ripple due to larger aggregation bandwidth configuration than ever, we suggest to allow [0.5]dB REFSENS relaxation as below:

Table 5.1.3-1: ΔRIB,c due to CA

|  |  |  |
| --- | --- | --- |
| Inter-band CA combination | Operating Band | ΔRIB,c (dB) |
| CA\_n96E | n96 | 0.5 |

## 5.2 CA\_2DL\_n2B\_1UL\_n2A

### 5.2.1 Channel bandwidths per operating band for CA

Table 5.2A.1-1: Intra-band contiguous CA operating bands in FR1

|  |  |
| --- | --- |
| NR CA Band | NR Band  (Table 5.2-1) |
| CA\_n2 | n2 |

Table 5.5A.1-1: NR CA configurations and bandwidth combination sets defined for intra-band contiguous CA

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NR CA configuration / Bandwidth combination set | | | | | | | | |
| NR CA configuration | Uplink CA configurations | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Maximum aggregated  bandwidth (MHz) | Bandwidth combination set |
| CA\_n2B | - | 5 | 15 |  |  |  | 20 | 0 |
|  |  | 10 | 10 |  |  |  |  |  |

### 5.2.2 UE maximum output power for Intra-band contiguous CA

Not needed as uplink is single CC.

### 5.2.3 UE additional maximum output power reduction for CA

Not needed as uplink is single CC.

### 5.2.4 Spurious emissions for UE co-existence for intra-band contiguous CA

Not needed as uplink is single CC.

### 5.2.5 Reference sensitivity power level for Intra-band contiguous CA

Not needed as PCC REFSENS is same as single carrier REFSENS and DL SCC is further away from UL than DL PCC.

### 5.2.6 In-band blocking

Table 7.6A.2.1-2a: In-band blocking for intra-band contiguous CA with FDL\_low < 2700 MHz and FUL\_low < 2700 MHz

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| NR band | Parameter | Unit | Case 1 | Case 2 |  |
|  | Pinterferer | dBm | -56 | -44 |  |
| n2 | Finterferer (offset) | MHz | -BWchannel CA/2 –FIoffset, case 1  and  BWchannel CA/2 +FIoffset, case 1 | ≤ -BWchannel CA/2 –FIoffset, case 2  and  ≥ BWchannel CA/2 +FIoffset, case 2 |  |
|  | Finterferer | MHz | NOTE 2 | FDL\_low – 15  to  FDL\_high + 15 |  |
|  | Finterferer | MHz | NOTE 2 | FDL\_low – 12  to  FDL\_high + 15 |  |
| NOTE 1: The absolute value of the interferer offset Finterferer (offset) shall be further adjusted to MHz with SCS the sub-carrier spacing of the carrier closest to the interferer in MHz. The interferer is an NR signal with 15 kHz SCS.  NOTE 2: For each carrier frequency, the requirement applies for two interferer carrier frequencies: a: -BWchannel CA/2 – FIoffset, case 1; b: BWchannel CA/2 + FIoffset, case 1  NOTE 3: BWchannel CA denotes the aggregated channel bandwidth of the wanted signal  NOTE 4: n48 follows the requirement in this frequency range according to the general requirement defined in Clause 7.1A. | | | | | |

### 5.2.7 Out-of-band blocking

Table 7.6A.3-2: Out of-band blocking for intra-band contiguous CA

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| NR band | Parameter | Unit | Range1 | Range 2 | Range 3 |
|  | Pinterferer | dBm | -45 | -30 | -15 |
| n2 | Finterferer (CW) | MHz | -60 < f – FDL\_low < -15  or  15 < f – FDL\_high < 60 | -85 < f – FDL\_low ≤ -60  or  60 ≤ f – FDL\_high < 85 | 1 ≤ f ≤ FDL\_low – 85  or  FDL\_high + 85 ≤ f  ≤ 12750 |
| NOTE 1: The power level of the interferer (PInterferer) for Range 3 shall be modified to -20 dBm for FInterferer > 6000 MHz.  NOTE 2: BWChannel\_CA denotes the aggregated channel bandwidth of the wanted signal  NOTE 3: The power level of the interferer (PInterferer) for Range 3 shall be modified to -20 dBm, for FInterferer > 2700 MHz and FInterferer < 4800 MHz. For BWChannel\_CA > 15 MHz, the requirement for Range 1 is not applicable and Range 2 applies from the frequency offset of 3\*BWChannel\_CA from the band edge. For BWChannel\_CA larger than 60 MHz, the requirement for Range 2 is not applicable and Range 3 applies from the frequency offset of 3\*BWChannel\_CA from the band edge.  NOTE 4: The power level of the interferer (PInterferer) for Range 3 shall be modified to -20 dBm, for FInterferer > 3650 MHz and FInterferer < 5750 MHz. For BWChannel\_CA≥ 40 MHz, the requirement for Range 2 is not applicable and Range 3 applies from the frequency offset of 3\*BWChannel\_CA from the band edge.  NOTE 5: The power level of the interferer (PInterferer) for Range 3 shall be modified to -20 dBm for FInterferer > 2700 MHz and FInterferer < 4800 MHz | | | | | |

### 5.2.8 Narrow band blocking

Table 7.6A.4.1-1: Narrow-band blocking for intra-band contiguous CA

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| NR band | Parameter | Unit | NR CA bandwidth class | |
|  |  |  | B | C |
| n2 | Pw in Transmission Bandwidth Configuration, per CC | dBm | REFSENS + NR CA Bandwidth Class specific value below | |
|  |  |  | 16 | 16 |
|  | Puw (CW) | dBm | -55 | -55 |
|  | Fuw (offset for*Df* = 15 kHz, 30 kHz) | MHz | - Foffset – 0.2  /  + Foffset + 0.2 | - Foffset – 0.2  /  + Foffset + 0.2 |
|  |  |  |  |  |
| NOTE 1: The transmitter shall be set a 4 dB below PCMAX\_L,f,c at the minimum UL configuration specified in Table 7.3.2-3 with PCMAX\_L,f,c defined in clause 6.2.4.  NOTE 2: Reference measurement channel is specified in Annexes A.3.2 and A3.2 with one sided dynamic OCNG Pattern OP.1 FDD/TDD as described in Annex A.5.1.1/A.5.2.1.  NOTE 3: The PREFSENS power level is specified in Table 7.3.2-1 and Table 7.3.2-2 for two and four antenna ports, respectively.  NOTE 4: The Fuw (offset) is the frequency separation of the center frequency of the carrier closest to the interferer and the center frequency of the interferer and shall be further adjusted to MHz to be offset from the sub-carrier raster. | | | | |

## 5.3 CA\_2DL\_n25B\_1UL\_n25A

### 5.3.1 Channel bandwidths per operating band for CA

Table 5.2A.1-1: Intra-band contiguous CA operating bands in FR1

|  |  |
| --- | --- |
| NR CA Band | NR Band  (Table 5.2-1) |
| CA\_n25 | n25 |

Table 5.5A.1-1: NR CA configurations and bandwidth combination sets defined for intra-band contiguous CA

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NR CA configuration / Bandwidth combination set | | | | | | | | |
| NR CA configuration | Uplink CA configurations | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Maximum aggregated  bandwidth (MHz) | Bandwidth combination set |
| CA\_n25B | - | 5 | 15 |  |  |  | 20 | 0 |
|  |  | 10 | 10 |  |  |  |  |  |

### 5.3.2 UE maximum output power for Intra-band contiguous CA

Not needed as uplink is single CC.

### 5.3.3 UE additional maximum output power reduction for CA

Not needed as uplink is single CC.

### 5.3.4 Spurious emissions for UE co-existence for intra-band contiguous CA

Not needed as uplink is single CC.

### 5.3.5 Reference sensitivity power level for Intra-band contiguous CA

Not needed as PCC REFSENS is same as single carrier REFSENS and DL SCC is further away from UL than DL PCC.

### 5.3.6 In-band blocking

Table 7.6A.2.1-2a: In-band blocking for intra-band contiguous CA with FDL\_low < 2700 MHz and FUL\_low < 2700 MHz

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| NR band | Parameter | Unit | Case 1 | Case 2 |  |
|  | Pinterferer | dBm | -56 | -44 |  |
| n25 | Finterferer (offset) | MHz | -BWchannel CA/2 –FIoffset, case 1  and  BWchannel CA/2 +FIoffset, case 1 | ≤ -BWchannel CA/2 –FIoffset, case 2  and  ≥ BWchannel CA/2 +FIoffset, case 2 |  |
|  | Finterferer | MHz | NOTE 2 | FDL\_low – 15  to  FDL\_high + 15 |  |
|  | Finterferer | MHz | NOTE 2 | FDL\_low – 12  to  FDL\_high + 15 |  |
| NOTE 1: The absolute value of the interferer offset Finterferer (offset) shall be further adjusted to MHz with SCS the sub-carrier spacing of the carrier closest to the interferer in MHz. The interferer is an NR signal with 15 kHz SCS.  NOTE 2: For each carrier frequency, the requirement applies for two interferer carrier frequencies: a: -BWchannel CA/2 – FIoffset, case 1; b: BWchannel CA/2 + FIoffset, case 1  NOTE 3: BWchannel CA denotes the aggregated channel bandwidth of the wanted signal  NOTE 4: n48 follows the requirement in this frequency range according to the general requirement defined in Clause 7.1A. | | | | | |

### 5.3.7 Out-of-band blocking

Table 7.6A.3-2: Out of-band blocking for intra-band contiguous CA

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| NR band | Parameter | Unit | Range1 | Range 2 | Range 3 |
|  | Pinterferer | dBm | -45 | -30 | -15 |
| n25 | Finterferer (CW) | MHz | -60 < f – FDL\_low < -15  or  15 < f – FDL\_high < 60 | -85 < f – FDL\_low ≤ -60  or  60 ≤ f – FDL\_high < 85 | 1 ≤ f ≤ FDL\_low – 85  or  FDL\_high + 85 ≤ f  ≤ 12750 |
| NOTE 1: The power level of the interferer (PInterferer) for Range 3 shall be modified to -20 dBm for FInterferer > 6000 MHz.  NOTE 2: BWChannel\_CA denotes the aggregated channel bandwidth of the wanted signal  NOTE 3: The power level of the interferer (PInterferer) for Range 3 shall be modified to -20 dBm, for FInterferer > 2700 MHz and FInterferer < 4800 MHz. For BWChannel\_CA > 15 MHz, the requirement for Range 1 is not applicable and Range 2 applies from the frequency offset of 3\*BWChannel\_CA from the band edge. For BWChannel\_CA larger than 60 MHz, the requirement for Range 2 is not applicable and Range 3 applies from the frequency offset of 3\*BWChannel\_CA from the band edge.  NOTE 4: The power level of the interferer (PInterferer) for Range 3 shall be modified to -20 dBm, for FInterferer > 3650 MHz and FInterferer < 5750 MHz. For BWChannel\_CA≥ 40 MHz, the requirement for Range 2 is not applicable and Range 3 applies from the frequency offset of 3\*BWChannel\_CA from the band edge.  NOTE 5: The power level of the interferer (PInterferer) for Range 3 shall be modified to -20 dBm for FInterferer > 2700 MHz and FInterferer < 4800 MHz | | | | | |

### 5.3.8 Narrow band blocking

Table 7.6A.4.1-1: Narrow-band blocking for intra-band contiguous CA

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| NR band | Parameter | Unit | NR CA bandwidth class | |
|  |  |  | B | C |
| n25 | Pw in Transmission Bandwidth Configuration, per CC | dBm | REFSENS + NR CA Bandwidth Class specific value below | |
|  |  |  | 16 | 16 |
|  | Puw (CW) | dBm | -55 | -55 |
|  | Fuw (offset for*Df* = 15 kHz, 30 kHz) | MHz | - Foffset – 0.2  /  + Foffset + 0.2 | - Foffset – 0.2  /  + Foffset + 0.2 |
|  |  |  |  |  |
| NOTE 1: The transmitter shall be set a 4 dB below PCMAX\_L,f,c at the minimum UL configuration specified in Table 7.3.2-3 with PCMAX\_L,f,c defined in clause 6.2.4.  NOTE 2: Reference measurement channel is specified in Annexes A.3.2 and A3.2 with one sided dynamic OCNG Pattern OP.1 FDD/TDD as described in Annex A.5.1.1/A.5.2.1.  NOTE 3: The PREFSENS power level is specified in Table 7.3.2-1 and Table 7.3.2-2 for two and four antenna ports, respectively.  NOTE 4: The Fuw (offset) is the frequency separation of the center frequency of the carrier closest to the interferer and the center frequency of the interferer and shall be further adjusted to MHz to be offset from the sub-carrier raster. | | | | |

## 5.4 CA\_2DL\_n77B\_1UL\_n77A

### 5.4.1 Channel bandwidths per operating band for CA

Table 5.2A.1-1: Intra-band contiguous CA operating bands in FR1

|  |  |
| --- | --- |
| NR CA Band | NR Band  (Table 5.2-1) |
| CA\_n77 | n77 |

Table 5.5A.1-1: NR CA configurations and bandwidth combination sets defined for intra-band contiguous CA

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NR CA configuration / Bandwidth combination set | | | | | | | | |
| NR CA configuration | Uplink CA configurations | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Maximum aggregated  bandwidth (MHz) | Bandwidth combination set |
| CA\_n77B | - | 20 | 25, 30, 40 |  |  |  | 60 | 0 |
|  |  | 25 | 30 |  |  |  |  |  |

### 5.4.2 UE maximum output power for Intra-band contiguous CA

Not needed as uplink is single CC.

### 5.4.3 UE additional maximum output power reduction for CA

Not needed as uplink is single CC.

### 5.4.4 Spurious emissions for UE co-existence for intra-band contiguous CA

Not needed as uplink is single CC.

### 5.4.5 Reference sensitivity power level for Intra-band contiguous CA

Not needed as PCC REFSENS is same as single carrier REFSENS and DL SCC is further away from UL than DL PCC.

### 5.4.6 In-band blocking

Already specified for n77.

### 5.4.7 Out-of-band blocking

Already specified for n77.

### 5.4.8 Narrow band blocking

Not needed for n77.

## 5.5 CA\_2DL\_n40B\_2UL\_n40B

### 5.5.1 Channel bandwidths per operating band for CA

Table 5.5.1-1: Intra-band contiguous CA operating bands in FR1

|  |  |
| --- | --- |
| NR CA Band | NR Band  (Table 5.2-1) |
| CA\_n40 | n40 |

Table 5.5.1-2: NR CA configurations and bandwidth combination sets defined for intra-band contiguous CA

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NR CA configuration / Bandwidth combination set | | | | | | | | |
| NR CA configuration | Uplink CA configurations | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Maximum aggregated  bandwidth (MHz) | Bandwidth combination set |
| CA\_n40B | CA\_n40B | 10,15, 20, 30, 40, 50, 60, 80 | 10, 15, 20, 30, 40, 50, 60, 80 |  |  |  | 100 | 1 |

### 5.5.2 UE maximum output power for Intra-band contiguous CA

Table 5.5.2-1: UE Power Class for intra-band contiguous CA

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NR CA Configuration | Class 1 (dBm) | Tolerance (dB) | Class 2 (dBm) | Tolerance (dB) | Class 3 (dBm) | Tolerance (dB) | Class 4 (dBm) | Tolerance (dB) |
| CA\_n40B |  |  |  |  | 23 | +2/-21 |  |  |
| NOTE 1: If all transmitted resource blocks over all component carriers are confined within FUL\_low and FUL\_low + 4 MHz or/and FUL\_high – 4 MHz and FUL\_high, the maximum output power requirement is relaxed by reducing the lower tolerance limit by 1.5 dB  NOTE 2: PPowerClass is the maximum UE power specified without taking into account the tolerance  NOTE 3: For intra-band contiguous carrier aggregation the maximum power requirement shall apply to the total transmitted power over all component carriers (per UE). | | | | | | | | |

### 5.5.3 UE additional maximum output power reduction for CA

Not needed as there are no additional emission requirements.

### 5.5.4 Spurious emissions for UE co-existence for intra-band contiguous CA

Table 5.5.4-1: Requirements for uplink intra-band contiguous carrier aggregation

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| NR CA combination | Spurious emission | | | | | | |
|  | Protected Band | Frequency range (MHz) | | | Maximum Level (dBm) | MBW (MHz) | NOTE |
| CA\_n40 | E-UTRA Band 1, 3, 5, 7, 8, 11, 18, 19, 20, 21, 22, 26, 27, 28, 31, 32, 33, 34, 38, 39, 41, 42, 43, 44, 45, 50, 51, 52, 65, 67, 68, 69, 72, 74, 75, 76,  NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 44 |
| NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 8 |
| NOTE 2: As exceptions, measurements with a level up to the applicable requirements defined in Table 6.5.3.1-2 are permitted for each assigned NR carrier used in the measurement due to 2nd, 3rd, 4th or 5th harmonic spurious emissions. Due to spreading of the harmonic emission the exception is also allowed for the first 1 MHz frequency range immediately outside the harmonic emission on both sides of the harmonic emission. This results in an overall exception interval centred at the harmonic emission of (2 MHz + N x LCRB x RBsize kHz), where N is 2, 3, 4, 5 for the 2nd, 3rd, 4th or 5th harmonic respectively. The exception is allowed if the measurement bandwidth (MBW) totally or partially overlaps the overall exception interval.  NOTE 8: Applicable when co-existence with PHS system operating in 1884.5 - 1915.7 MHz.  NOTE 44: As exceptions, for 90 and 100 MHz aggregated bandwidth, -40 dBm/MHz is applicable in the frequency range of 2496 – 2505 MHz. | | | | | | | |

### 5.5.5 Reference sensitivity power level for Intra-band contiguous CA

Not needed as TDD band.

### 5.5.6 In-band blocking

Already captured in specification for n40

### 5.5.7 Out-of-band blocking

Already captured in specification for n40

### 5.5.8 Narrow band blocking

Already captured in specification for n40

## 5.6 CA\_2DL\_n3B\_1UL\_n3A

### 5.6.1 Channel bandwidths per operating band for CA

Table 5.6.1-1: Intra-band contiguous CA operating bands in FR1

|  |  |
| --- | --- |
| NR CA Band | NR Band  (Table 5.2-1) |
| CA\_n3 | n3 |

Table 5.6.1-1: NR CA configurations and bandwidth combination sets defined for intra-band contiguous CA

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NR CA configuration / Bandwidth combination set | | | | | | | | |
| NR CA configuration | Uplink CA configurations | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Maximum aggregated  bandwidth (MHz) | Bandwidth combination set |
| CA\_n3B | - | 5 | 15, 20, 25, 30 |  |  |  | 60 | 0 |
|  |  | 10 | 10, 15, 20, 25, 30 |  |  |  |  |  |
|  |  | 15, 20, 25, 30 | 5, 10, 15, 20, 25, 30 |  |  |  |  |  |

### 5.6.2 UE maximum output power for Intra-band contiguous CA

Not needed as uplink is single CC.

### 5.6.3 UE additional maximum output power reduction for CA

Not needed as uplink is single CC.

### 5.6.4 Spurious emissions for UE co-existence for intra-band contiguous CA

Not needed as uplink is single CC.

### 5.6.5 Reference sensitivity power level for Intra-band contiguous CA

Based on the REFSENS requirements for intra-hand contiguous CA specified in clause 7.3A.2.1 from TS 38.101-1, exceptions are not needed as PCC REFSENS is same as single carrier REFSENS and DL SCC is further away from UL than DL PCC.

### 5.6.6 In-band blocking

Table 5.6.6-1: In-band blocking for intra-band contiguous CA with FDL\_low < 2700 MHz and FUL\_low < 2700 MHz

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| NR band | Parameter | Unit | Case 1 | Case 2 |  |
|  | Pinterferer | dBm | -56 | -44 |  |
| n3 | Finterferer (offset) | MHz | -BWchannel CA/2 –FIoffset, case 1  and  BWchannel CA/2 +FIoffset, case 1 | ≤ -BWchannel CA/2 –FIoffset, case 2  and  ≥ BWchannel CA/2 +FIoffset, case 2 |  |
|  | Finterferer | MHz | NOTE 2 | FDL\_low – 15  to  FDL\_high + 15 |  |
|  | Finterferer | MHz | NOTE 2 | FDL\_low – 12  to  FDL\_high + 15 |  |
| NOTE 1: The absolute value of the interferer offset Finterferer (offset) shall be further adjusted to MHz with SCS the sub-carrier spacing of the carrier closest to the interferer in MHz. The interferer is an NR signal with 15 kHz SCS.  NOTE 2: For each carrier frequency, the requirement applies for two interferer carrier frequencies: a: -BWchannel CA/2 – FIoffset, case 1; b: BWchannel CA/2 + FIoffset, case 1  NOTE 3: BWchannel CA denotes the aggregated channel bandwidth of the wanted signal  NOTE 4: n48 follows the requirement in this frequency range according to the general requirement defined in Clause 7.1A. | | | | | |

### 5.6.7 Out-of-band blocking

Table 5.6.7-1: Out of-band blocking for intra-band contiguous CA

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| NR band | Parameter | Unit | Range1 | Range 2 | Range 3 |
|  | Pinterferer | dBm | -45 | -30 | -15 |
| n3 | Finterferer (CW) | MHz | -60 < f – FDL\_low < -15  or  15 < f – FDL\_high < 60 | -85 < f – FDL\_low ≤ -60  or  60 ≤ f – FDL\_high < 85 | 1 ≤ f ≤ FDL\_low – 85  or  FDL\_high + 85 ≤ f  ≤ 12750 |
| NOTE 1: The power level of the interferer (PInterferer) for Range 3 shall be modified to -20 dBm for FInterferer > 6000 MHz.  NOTE 2: BWChannel\_CA denotes the aggregated channel bandwidth of the wanted signal  NOTE 3: The power level of the interferer (PInterferer) for Range 3 shall be modified to -20 dBm, for FInterferer > 2700 MHz and FInterferer < 4800 MHz. For BWChannel\_CA > 15 MHz, the requirement for Range 1 is not applicable and Range 2 applies from the frequency offset of 3\*BWChannel\_CA from the band edge. For BWChannel\_CA larger than 60 MHz, the requirement for Range 2 is not applicable and Range 3 applies from the frequency offset of 3\*BWChannel\_CA from the band edge.  NOTE 4: The power level of the interferer (PInterferer) for Range 3 shall be modified to -20 dBm, for FInterferer > 3650 MHz and FInterferer < 5750 MHz. For BWChannel\_CA≥ 40 MHz, the requirement for Range 2 is not applicable and Range 3 applies from the frequency offset of 3\*BWChannel\_CA from the band edge.  NOTE 5: The power level of the interferer (PInterferer) for Range 3 shall be modified to -20 dBm for FInterferer > 2700 MHz and FInterferer < 4800 MHz | | | | | |

### 5.6.8 Narrow band blocking

Table 5.6.8-1: Narrow-band blocking for intra-band contiguous CA

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| NR band | Parameter | Unit | NR CA bandwidth class | |
|  |  |  | B | C |
| n3 | Pw in Transmission Bandwidth Configuration, per CC | dBm | REFSENS + NR CA Bandwidth Class specific value below | |
|  |  |  | 16 | 16 |
|  | Puw (CW) | dBm | -55 | -55 |
|  | Fuw (offset for*Df* = 15 kHz, 30 kHz) | MHz | - Foffset – 0.2  /  + Foffset + 0.2 | - Foffset – 0.2  /  + Foffset + 0.2 |
|  |  |  |  |  |
| NOTE 1: The transmitter shall be set a 4 dB below PCMAX\_L,f,c at the minimum UL configuration specified in Table 7.3.2-3 with PCMAX\_L,f,c defined in clause 6.2.4.  NOTE 2: Reference measurement channel is specified in Annexes A.3.2 and A3.2 with one sided dynamic OCNG Pattern OP.1 FDD/TDD as described in Annex A.5.1.1/A.5.2.1.  NOTE 3: The PREFSENS power level is specified in Table 7.3.2-1 and Table 7.3.2-2 for two and four antenna ports, respectively.  NOTE 4: The Fuw (offset) is the frequency separation of the center frequency of the carrier closest to the interferer and the center frequency of the interferer and shall be further adjusted to MHz to be offset from the sub-carrier raster. | | | | |

## 5.7 CA\_2DL\_n38B\_1UL\_n38A

### 5.7.1 Channel bandwidths per operating band for CA

Table 5.7.1-1: Intra-band contiguous CA operating bands in FR1

|  |  |
| --- | --- |
| NR CA Band | NR Band  (Table 5.2-1) |
| CA\_n38 | n38 |

Table 5.7.1-1: NR CA configurations and bandwidth combination sets defined for intra-band contiguous CA

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NR CA configuration / Bandwidth combination set | | | | | | | | |
| NR CA configuration | Uplink CA configurations | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Maximum aggregated  bandwidth (MHz) | Bandwidth combination set |
| CA\_n38B | - | 5 | 15, 20, 25 |  |  |  | 50 | 0 |
|  |  | 10 | 10, 15, 20, 25 |  |  |  |  |  |
|  |  | 15, 20, 25 | 5, 10, 15, 20, 25 |  |  |  |  |  |

### 5.7.2 UE maximum output power for Intra-band contiguous CA

Not needed as uplink is single CC.

### 5.7.3 UE additional maximum output power reduction for CA

Not needed as uplink is single CC.

### 5.7.4 Spurious emissions for UE co-existence for intra-band contiguous CA

Not needed as uplink is single CC.

### 5.7.5 Reference sensitivity power level for Intra-band contiguous CA

There is no REFSENS exception for this TDD intra-band contiguous CA band combination.

### 5.7.6 In-band blocking

Table 5.7.6-1: In-band blocking for intra-band contiguous CA with FDL\_low < 2700 MHz and FUL\_low < 2700 MHz

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| NR band | Parameter | Unit | Case 1 | Case 2 |  |
|  | Pinterferer | dBm | -56 | -44 |  |
| n38 | Finterferer (offset) | MHz | -BWchannel CA/2 –FIoffset, case 1  and  BWchannel CA/2 +FIoffset, case 1 | ≤ -BWchannel CA/2 –FIoffset, case 2  and  ≥ BWchannel CA/2 +FIoffset, case 2 |  |
|  | Finterferer | MHz | NOTE 2 | FDL\_low – 15  to  FDL\_high + 15 |  |
|  | Finterferer | MHz | NOTE 2 | FDL\_low – 12  to  FDL\_high + 15 |  |
| NOTE 1: The absolute value of the interferer offset Finterferer (offset) shall be further adjusted to MHz with SCS the sub-carrier spacing of the carrier closest to the interferer in MHz. The interferer is an NR signal with 15 kHz SCS.  NOTE 2: For each carrier frequency, the requirement applies for two interferer carrier frequencies: a: -BWchannel CA/2 – FIoffset, case 1; b: BWchannel CA/2 + FIoffset, case 1  NOTE 3: BWchannel CA denotes the aggregated channel bandwidth of the wanted signal  NOTE 4: n48 follows the requirement in this frequency range according to the general requirement defined in Clause 7.1A. | | | | | |

### 5.7.7 Out-of-band blocking

Table 5.7.7-1: Out of-band blocking for intra-band contiguous CA

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| NR band | Parameter | Unit | Range1 | Range 2 | Range 3 |
|  | Pinterferer | dBm | -45 | -30 | -15 |
| n38 | Finterferer (CW) | MHz | -60 < f – FDL\_low < -15  or  15 < f – FDL\_high < 60 | -85 < f – FDL\_low ≤ -60  or  60 ≤ f – FDL\_high < 85 | 1 ≤ f ≤ FDL\_low – 85  or  FDL\_high + 85 ≤ f  ≤ 12750 |
| NOTE 1: The power level of the interferer (PInterferer) for Range 3 shall be modified to -20 dBm for FInterferer > 6000 MHz.  NOTE 2: BWChannel\_CA denotes the aggregated channel bandwidth of the wanted signal  NOTE 3: The power level of the interferer (PInterferer) for Range 3 shall be modified to -20 dBm, for FInterferer > 2700 MHz and FInterferer < 4800 MHz. For BWChannel\_CA > 15 MHz, the requirement for Range 1 is not applicable and Range 2 applies from the frequency offset of 3\*BWChannel\_CA from the band edge. For BWChannel\_CA larger than 60 MHz, the requirement for Range 2 is not applicable and Range 3 applies from the frequency offset of 3\*BWChannel\_CA from the band edge.  NOTE 4: The power level of the interferer (PInterferer) for Range 3 shall be modified to -20 dBm, for FInterferer > 3650 MHz and FInterferer < 5750 MHz. For BWChannel\_CA≥ 40 MHz, the requirement for Range 2 is not applicable and Range 3 applies from the frequency offset of 3\*BWChannel\_CA from the band edge.  NOTE 5: The power level of the interferer (PInterferer) for Range 3 shall be modified to -20 dBm for FInterferer > 2700 MHz and FInterferer < 4800 MHz | | | | | |

### 5.7.8 Narrow band blocking

Table 5.7.8-1: Narrow-band blocking for intra-band contiguous CA

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| NR band | Parameter | Unit | NR CA bandwidth class | |
|  |  |  | B | C |
| n38 | Pw in Transmission Bandwidth Configuration, per CC | dBm | REFSENS + NR CA Bandwidth Class specific value below | |
|  |  |  | 16 | 16 |
|  | Puw (CW) | dBm | -55 | -55 |
|  | Fuw (offset for*f* = 15 kHz, 30 kHz) | MHz | - Foffset – 0.2  /  + Foffset + 0.2 | - Foffset – 0.2  /  + Foffset + 0.2 |
|  |  |  |  |  |
| NOTE 1: The transmitter shall be set a 4 dB below PCMAX\_L,f,c at the minimum UL configuration specified in Table 7.3.2-3 with PCMAX\_L,f,c defined in clause 6.2.4.  NOTE 2: Reference measurement channel is specified in Annexes A.3.2 and A3.2 with one sided dynamic OCNG Pattern OP.1 FDD/TDD as described in Annex A.5.1.1/A.5.2.1.  NOTE 3: The PREFSENS power level is specified in Table 7.3.2-1 and Table 7.3.2-2 for two and four antenna ports, respectively.  NOTE 4: The Fuw (offset) is the frequency separation of the center frequency of the carrier closest to the interferer and the center frequency of the interferer and shall be further adjusted to MHz to be offset from the sub-carrier raster. | | | | |

# 6 Intra-Band Non-Contiguous Carrier Aggregation FR1: Specific Band Combination Part

## 6.1 CA\_2DL\_n71(2A)\_1UL\_n71A

### 6.1.1 Channel bandwidths per operating band for CA

Table 6.1.1-1: Supported bandwidth combinations for CA\_n71(2A)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| NR CA Configuration | Uplink Configurations | Channel bandwidths for carrier  (MHz) | Channel bandwidths for carrier  (MHz) | Channel bandwidths for carrier  (MHz) | Channel bandwidths for carrier  (MHz) | Maximum  Aggregated bandwidth  (MHz) | Bandwidth combination set |
| CA\_n71(2A) | - | 5,10,15,20 | 5,10,15, 20 |  |  | 30 | 0 |

### 6.1.2 UE co-existence studies

There are no co-existence issues for this combination.

### 6.1.3 REFSENS

REFSENS for CA\_n71(2A) need to be added in below table of TS 38.101-1. MSD values proposed are tentative values for the RAN4 #96 meeting, and these will be crosschecked and to be concluded at the following RAN4 meeting.

Table 7.3A.2.2-1: Intra-band non-contiguous CA with one uplink configuration for reference sensitivity

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| CA configuration | SCS  (kHz) | Aggregated channel bandwidth (PCC+SCC) | Wgap / [MHz] | UL PCC allocation | ΔRIBNC (dB) | Duplex mode |
| CA\_n71(2A) | 15 | 25RB+25RB | Wgap = 25.0 | 5 | 4.0 | FDD |
| Wgap = 5.0 | 20 | 0.0 |
| 50RB+25RB | Wgap = 20.0 | 51 | 4.6 |
| Wgap = 5.0 | 201 | 2.3 |
| 75RB+50RB | Wgap = 10.0 | 52 | 22.2 |
| Wgap = 5.0 | 203 | 5.2 |
| Note 1: Uplink resource block starts at RB postion [9] for SCS=15KHz.  Note 2: Uplink resource block starts at RB postion [2] for SCS=15KHz.  Note 3: Uplink resource block starts at RB postion [19] for SCS=15KHz. | | | | | | |

## 6.2 CA\_2DL\_n2(2A)\_1UL\_n2A

### 6.2.1 Channel bandwidths per operating band for CA

Table 6.2.1-1: Supported bandwidth combinations for CA\_2DL\_n2(2A)\_1UL \_n2A

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | E-UTRA CA configuration / Bandwidth combination set | | | | | | |
| NR CA configuration | Uplink CA configurations | Component carriers in order of increasing carrier frequency | | | | | Maximum aggregated  bandwidth [MHz] | Bandwidth combination set |
| Channel bandwidths for carrier [MHz] | Channel bandwidths for carrier [MHz] | Channel bandwidths for carrier [MHz] | Channel bandwidths for carrier [MHz] | Channel bandwidths for carrier [MHz] |
| CA\_n2(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20 |  |  |  | 40 | 0 |

### 6.2.2 Co-existence studies

There are no co-existence issues for this combination.

### 6.2.3 REFSENS

REFSENS can be impacted by the PCC UL being closer to do the SCC DL than the nominal spacing. REFSENS values are same as for CA\_n2(2A).

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CA configuration** | **SCS**  **kHz** | **Aggregated channel bandwidth (PCC+SCC)** | **Wgap / [MHz]** | **UL PCC allocation** | **ΔRIBNC (dB)** | **Duplex mode** |
| CA\_n2(2A) | 15 | 25RB+25RB | Wgap = 55.0 | 101 | 5.0 | FDD |
| Wgap = 30.0 | 25 | 0.0 |
| NOTE 1: 1 refers to the UL resource blocks shall be located as close as possible to the downlink operating band but confined within the transmission.  NOTE 2: Wgap is the sub-block gap between the two sub-blocks.  NOTE 3: The carrier centre frequency of SCC in the DL operating band is configured closer to the UL operating band. | | | | | | |

## 6.3 CA\_2DL\_n5(2A)\_1UL\_n5A

### 6.3.1 Channel bandwidths per operating band for CA

Table 6.3.1-1: Supported bandwidth combinations for CA\_n5(2A)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| NR CA Configuration | Uplink Configurations | Channel bandwidths for carrier  (MHz) | Channel bandwidths for carrier  (MHz) | Channel bandwidths for carrier  (MHz) | Channel bandwidths for carrier  (MHz) | Maximum  Aggregated bandwidth  (MHz) | Bandwidth combination set |
| CA\_n5(2A) | - | 5,10,15,20 | 5,10,15, 20 |  |  | 25 | 0 |

### 6.3.2 UE co-existence studies

There are no co-existence issues for this combination.

### 6.3.3 REFSENS

Below analysis assumptions are used in the REFSENS analysis.

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Value** | **Unit** |
| CIM5 | -70 | dBc |
| n5 filter T/R isolation | 53 | dB |
| Front-end loss | 4 | dB |
| Thermal noise at n5 RX ANT port | -165 | dBm/Hz |
| Transceiver effective phase noise | -140 | dBc/Hz |
| SNR requirement for QPSK | -1 | dB |

REFSENS for CA\_n5(2A) need to be added in below table of TS 38.101-1.

Table 7.3A.2.2-1: Intra-band non-contiguous CA with one uplink configuration for reference sensitivity

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| CA configuration | SCS  (kHz) | Aggregated channel bandwidth (PCC+SCC) | Wgap / [MHz] | UL PCC allocation | ΔRIBNC (dB) | Duplex mode |
| CA\_n5(2A) | 15 | 75RB + 25RB | Wgap = 5.0 | 55 | 6.3 | FDD |
| NOTE 5: Refers to the UL resource blocks shall be located as close as possible to the downlink operating band but confined within the transmission. | | | | | | |

## 6.4 CA\_3DL\_n77(3A)\_1UL\_n77A

### 6.4.1 Channel bandwidths per operating band for CA

Table 6.4.1-1: Supported bandwidth combinations for CA\_3DL\_n77(3A)\_1UL \_n77A

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| NR CA Configuration | Uplink Configurations | Channel bandwidths for carrier  [MHz] | Channel bandwidths for carrier  [MHz] | Channel bandwidths for carrier  [MHz] | Aggregated bandwidth  [MHz] | Bandwidth combination set |
| CA\_n77(3A) | - | 20, 40, 80, 100 | 20, 40, 80, 100 | 20, 40, 80, 100 | 300 | 0 |
| 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 300 | 1 |

### 6.4.2 Co-existence studies

There are no additional co-existence issues for this combination.

### 6.4.3 REFSENS

There are no REFSENS exceptions for this combination.

## 6.5 CA\_2DL\_n96(2A)\_1UL\_n96A

### 6.5.1 Channel bandwidths per operating band for CA

Table 6.5.1-1: Supported bandwidth combinations for CA\_n96(2A)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| NR CA Configuration | Uplink Configurations | Channel bandwidths for carrier  (MHz) | Channel bandwidths for carrier  (MHz) | Channel bandwidths for carrier  (MHz) | Channel bandwidths for carrier  (MHz) | Maximum  Aggregated bandwidth  (MHz) | Bandwidth combination set |
| CA\_n96(2A) | - | 20, 40, 60, 80 | 20, 40, 60, 80 |  |  | 160 | 0 |

### 6.5.2 UE co-existence studies

There are no co-existence issues for this combination.

### 6.5.3 REFSENS

There are no REFSENS exceptions for this combination.

## 6.6 CA\_2DL\_n96(3A)\_1UL\_n96A

### 6.6.1 Channel bandwidths per operating band for CA

Table 6.6.1-1: Supported bandwidth combinations for CA\_n96(3A)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| NR CA Configuration | Uplink Configurations | Channel bandwidths for carrier  (MHz) | Channel bandwidths for carrier  (MHz) | Channel bandwidths for carrier  (MHz) | Channel bandwidths for carrier  (MHz) | Maximum  Aggregated bandwidth  (MHz) | Bandwidth combination set |
| CA\_n96(3A) | - | 20, 40, 60, 80 | 20, 40, 60, 80 | 20, 40, 60, 80 |  | 240 | 0 |

### 6.6.2 UE co-existence studies

There are no co-existence issues for this combination.

### 6.6.3 REFSENS

There are no REFSENS exceptions for this combination.

## 6.7 CA\_2DL\_n96(4A)\_1UL\_n96A

### 6.7.1 Channel bandwidths per operating band for CA

Table 6.7.1-1: Supported bandwidth combinations for CA\_n96(4A)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| NR CA Configuration | Uplink Configurations | Channel bandwidths for carrier  (MHz) | Channel bandwidths for carrier  (MHz) | Channel bandwidths for carrier  (MHz) | Channel bandwidths for carrier  (MHz) | Maximum  Aggregated bandwidth  (MHz) | Bandwidth combination set |
| CA\_n96(4A) | - | 20, 40, 60, 80 | 20, 40, 60, 80 | 20, 40, 60, 80 | 20, 40, 60, 80 | 320 | 0 |

### 6.7.2 UE co-existence studies

There are no co-existence issues for this combination.

### 6.7.3 REFSENS

The DL NCCA with four carriers CA\_n96(4A) was first required in RAN4. Considering design complexity of four non-contiguous carriers, REFSENS relaxation may be needed. One possible implantation is split receiver architecture to cover non-contiguous carriers within the whole pass band. Here we propose ΔRIBNC as below:

Table 6.7.3-1: Intra-band non-contiguous CA reference sensitivity for shared spectrum

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| CA configuration | SCS  (PCC/SCC)  (kHz) | Aggregated channel bandwidth (PCC+SCC) | ΔRIBNC (dB) | Duplex mode |
| CA\_n96(4A) | 15/30/60 | 320MHz | 0.5 | TDD |

## 6.8 CA\_2DL\_n12(2A)\_1UL\_n12A

### 6.8.1 Channel bandwidths per operating band for CA

Table 5.2A.1-1: Intra-band contiguous CA operating bands in FR1

|  |  |
| --- | --- |
| NR CA Band | NR Band  (Table 5.2-1) |
| CA\_n12(\*) | n12 |

Table 5.5A.1-1: NR CA configurations and bandwidth combination sets defined for intra-band contiguous CA

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NR CA configuration / Bandwidth combination set | | | | | | | | |
| NR CA configuration | Uplink CA configurations | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Maximum aggregated  bandwidth (MHz) | Bandwidth combination set |
| CA\_n12(2A) | - | 5 | 5 |  |  |  | 10 | 0 |

### 6.8.2 UE maximum output power for Intra-band contiguous CA

Not needed as uplink is single CC.

### 6.8.3 UE additional maximum output power reduction for CA

Not needed as uplink is single CC.

### 6.8.4 Spurious emissions for UE co-existence for intra-band contiguous CA

Not needed as uplink is single CC.

### 6.8.5 Reference sensitivity power level for Intra-band contiguous CA

MDS is re-used from CA\_12A-12A.

Table 7.3A.2.2-1: Intra-band non-contiguous CA with one uplink configuration for reference sensitivity in FDD bands.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CA configuration** | **SCS**  **kHz** | **Aggregated channel bandwidth (PCC+SCC)** | **Wgap / [MHz]** | **UL PCC allocation** | **ΔRIBNC (dB)** | **Duplex mode** |
| CA\_n12(2A) | 15/15 | 5MHz + 5MHz | 0.0 < Wgap ≤ 7.0 | 5(RBstart=12) | 3 | FDD |
| NOTE 1: 1 refers to the UL resource blocks shall be located as close as possible to the downlink operating band but confined within the transmission.  NOTE 2: Wgap is the sub-block gap between the two sub-blocks.  NOTE 3: The carrier centre frequency of SCC in the DL operating band is configured closer to the UL operating band. | | | | | | |

### 6.8.6 In-band blocking

Not needed requirement refers back to single carrier requirement.

### 6.8.7 Out-of-band blocking

Not needed requirement refers back to single carrier requirement.

### 6.8.8 Narrow band blocking

Not needed requirement refers back to single carrier requirement.

## 6.9 CA\_2DL\_n25(2A)\_1UL\_n25A CA\_3DL\_n25(3A)\_1UL\_n25A

### 6.9.1 Channel bandwidths per operating band for CA

Table 6.9.1-1: Supported bandwidth combinations

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | E-UTRA CA configuration / Bandwidth combination set | | | | | | |
| NR CA configuration | Uplink CA configurations | Component carriers in order of increasing carrier frequency | | | | | Maximum aggregated  bandwidth [MHz] | Bandwidth combination set |
| Channel bandwidths for carrier [MHz] | Channel bandwidths for carrier [MHz] | Channel bandwidths for carrier [MHz] | Channel bandwidths for carrier [MHz] | Channel bandwidths for carrier [MHz] |
| CA\_n25(2A) | - | 5, 10, 15, 20, 25, 30, 40 | 5, 10, 15, 20, 25, 30, 40 |  |  |  | 60 | 1 |
| CA\_n25(3A) | - | 5, 10, 15, 20, 25, 30, 40 | 5, 10, 15, 20, 25, 30, 40 | 5, 10, 15, 20, 25, 30, 40 |  |  | 55 | 0 |

### 6.9.2 REFSENS

Table 6.9.2-1: MSD values

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CA configuration** | SCS  (PCC/SCC)  (kHz) | **Aggregated channel bandwidth (PCC+SCC)** | **Wgap / [MHz]** | **UL PCC allocation** | **ΔRIBNC (dB)** | **Duplex mode** |
| CA\_n25(2A) CA\_n25(3A) | 15/15 | 40MHz + 5MHz | Wgap = 20.0 | 40 (RBstart = 176) | [24.6]11 | FDD |
| NOTE 11: For operation with three or more non-contiguous component carriers, ΔRIBNC applies to all secondary component carriers | | | | | | |

## 6.10 CA\_2DL\_n41(2A)\_1UL\_n41A CA\_2DL\_n41(A-C)\_1UL\_n41A CA\_3DL\_n41(3A)\_1UL\_n41A

### 6.10.1 Channel bandwidths per operating band for CA

Table 6.10.1-1: Supported bandwidth combinations for CA\_2DL\_n41(xA)\_1UL \_n41A

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | E-UTRA CA configuration / Bandwidth combination set | | | | | | |
| NR CA configuration | Uplink CA configurations | Component carriers in order of increasing carrier frequency | | | | | Maximum aggregated  bandwidth [MHz] | Bandwidth combination set |
| Channel bandwidths for carrier [MHz] | Channel bandwidths for carrier [MHz] | Channel bandwidths for carrier [MHz] | Channel bandwidths for carrier [MHz] | Channel bandwidths for carrier [MHz] |
| CA\_n41(2A) | - | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |  |  | 190 | 3 |
| CA\_n41(3A) | - | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |  | 190 | 0 |
| CA\_n41(A-C) |  | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | See CA\_n41C Bandwidth Combination Set 2 in Table 5.5A.1-1 |  |  |  | 190 | 0 |

### 6.10.2 REFSENS

Since n41 is TDD there is no need to define additional REFSENS requirements.

## 6.11 CA\_2DL\_n1(2A)\_1UL\_n1A

### 6.11.1 Channel bandwidths per operating band for CA

Table 6.11.1-1: Supported bandwidth combinations

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| NR CA Configuration | Uplink Configurations | Channel bandwidths for carrier  [MHz] | Channel bandwidths for carrier  [MHz] | Channel bandwidths for carrier  [MHz] | Aggregated bandwidth  [MHz] | Bandwidth combination set |
| CA\_n1(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20 |  | 40 | 0 |

### 6.11.2 Co-existence studies

There are no additional co-existence issues for this combination since it is single UL.

### 6.11.3 REFSENS

This combination requires MSD.

Table 7.3A.2.2-1: Intra-band non-contiguous CA with one uplink configuration for reference sensitivity in FDD bands.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| CA configuration | SCS  (PCC/SCC)  (kHz) | Aggregated channel bandwidth (PCC+SCC) | Wgap / [MHz] | UL PCC allocation  (LCRB) | ΔRIBNC (dB) | Duplex mode |
| CA\_n1(2A) | 15/15 | 5MHz + 5MHz | 0.0 < Wgap ≤ 50.0 | 25 | 0.5 | FDD |

# 7 Intra-Band Contiguous Carrier Aggregation FR2: Specific Band Combination Part

## 7.1 CA\_xDL\_a\_yUL\_b

### 7.1.1 Channel bandwidths per operating band for CA

<Text will be added.>

### 7.1.2 UE co-existence studies

<Text will be added.>

# 8 Intra-Band Non-Contiguous Carrier Aggregation FR2: Specific Band Combination Part

## 8.1 CA\_xDL\_a-a\_yUL\_b-b

### 8.1.1 Channel bandwidths per operating band for CA

<Text will be added.>

### 8.1.2 UE co-existence studies

<Text will be added.>

# Annex A - Change history

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Date** | **Meeting** | **TDoc** | **Subject/Comment** | **New version** |
| 2020-08 | 3GPP RAN4#96-e | R4-2010680 | TR skeleton | 0.0.1 |
| 2020-08 | 3GPP RAN4#96-e | R4-2011888 | Implemented TP’s from RAN4 #96-e:  R4-2011619, “TP to TR 38.717-01-01 to include CA\_n71(2A)”, Ericsson, T-Mobile US | 0.1.0 |
| 2020-11 | 3GPP RAN4#97-e | R4-2015924 | Implemented TP’s from RAN4 #97-e:  R4-2016329. “TP to TR 38.717-01-01 to include CA\_n2(2A)”, Ericsson, Verizon  R4-2016679, “TP to TR 38.717-01-01 to include CA\_n5(2A)”, Ericsson, Verizon, MediaTek  R4-2016339, “TP to TR 38.717-01-01 to update MSD values CA\_n71(2A)”, Ericsson, T-Mobile US | 0.2.0 |
| 2021-02 | 3GPP RAN4#98-e | R4-2101891 | Implemented TP from RAN4 #98-e:  R4-2100708, “TP for TR 38.717-01-01: CA\_3DL\_n77(3A)\_1UL\_n77A”, SoftBank Corp. | 0.3.0 |
| 2021-04 | 3GPP RAN4#98-bis-e | R4-2106704 | Implemented TP from RAN4 #98-bis-e:  R4-2106648, “Updated TP for TR 38.717-01-01: CA\_n77(3A)\_BCS1”, Huawei, HiSilicon | 0.4.0 |
| 2021-05 | 3GPP RAN4#99-e | R4-2111079 | No new TP’s to implement from RAN4 #99-e | 0.5.0 |
| 2021-08 | 3GPP RAN4#100-e | R4-2113562 | No new TP’s to implement from RAN4 #100-e | 0.6.0 |
| 2021-11 | 3GPP RAN4#101-e | R4-2118494 | Implemented TP’s from RAN4 #101-e:  R4-2119799, TP to TR 38.717.01-01 for NR intra band CA\_n96, Charter Communications, Inc  R4-2119804 TP to TR 38.717-01-01: CA\_n2B, Nokia, US Cellular  R4-2119805, TP to TR 38.717-01-01: CA\_n25B, Nokia, US Cellular  R4-2117583, TP to TR 38.717-01-01: CA\_n77B, Nokia, US Cellular  R4-2117584, TP to TR 38.717-01-01: CA\_n12(2A), Nokia, US Cellular  R4-2119820, TP for 38.717-01-01 to add CA\_n25(2A) and CA\_n25(3A), Ericsson, T-Mobile US  R4-2119821, TP for 38.717-01-01 to add CA\_n41(2A), CA\_n41(3A) and CA\_n41(A-C), Ericsson, T-Mobile US  R4-2119824, TP to TR 38.717-01-01 Addition of CA\_n1(2A), Nokia | 0.7.0 |
| 2022-02 | 3GPP RAN4#102-e | R4-2205684 | Implemented TP’s from RAN4 #101-bis-e:  [R4-2202174](https://www.3gpp.org/ftp/tsg_ran/WG4_Radio/TSGR4_101-bis-e/Docs/R4-2202174.zip), TP to TR 38.717-01-01 Addition of CA\_n40B, Nokia, NBN  Implemented TP’s from RAN4 #102-e:  R4-2206270, TP for TR 38.717-01-01 CA\_n3B\_BCS0, Huawei, HiSilicon  R4-2206271, TP for TR 38.717-01-01 CA\_n38B\_BCS0, Huawei, HiSilicon | 0.8.0 |
| 2022-05 | 3GPP RAN4#103-e | R4-2209551 | No new TP’s at RAN4 #103-e | 0.9.0 |
| 2022-06 | 3GPP RAN #96 | RP-221323 | Presented for approval at RAN plenary. | 1.0.0 |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2022-06 | RAN#96 |  |  |  |  | Approved by plenary – Rel-17 spec under change control | 17.0.0 |